                                       
                                                Waste Water Treatment 
1. Primary treatment – removes solid waste by sedimentation.
a. Screening  - removal of large object 
b. Grit and sand removal -  removal of sand pebbles , grit 
c. Primary sedimentation –a) primary sludge separation at the bottom - digester tank – anaerobic bacteriabiogas , manure – 
b) Clarified water is obtained after the removal of  sludge and floating impurities 
2.  Secondary treatment  ( biological process) – bacteria break down dissolved waste.
a. Aeration   b. secondary sedimentation   
3.  Tertiary treatment – filtration and disinfection make water safe by Chlorine or ozone 
[image: ]
image1.png
Preliminary

waste water
from sewer

Secondary

Tertiary

filtration and
chlorination

screening
of large solids

activated sludge
passes to digester

=

effluent
discharge

sludge methane gas

digester




